<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0.016" x2="22.86" y2="0.016" width="0.2032" layer="20"/>
<wire x1="22.86" y1="0.016" x2="22.86" y2="43.18" width="0.2032" layer="20"/>
<wire x1="22.86" y1="43.18" x2="0" y2="43.18" width="0.2032" layer="20"/>
<wire x1="0" y1="43.18" x2="0" y2="0.016" width="0.2032" layer="20"/>
<text>Servo Trigger</text>
<text>A</text>
<text>B</text>
<text>T</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>SIG\</text>
<text>IN</text>
<text>ISP</text>
<text>GND</text>
<text>SJ1-Mode</text>
<text>SJ2-Input Polarity</text>
<text>BLK</text>
<text>RED</text>
<text>WHT</text>
<text>BRN</text>
<text>ORG</text>
<text>RED</text>
<text>GND</text>
<text>VCC</text>
<text>IN</text>
<text>GND</text>
<text>ISP</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>SIG\</text>
<text>VCC</text>
<text>GND</text>
<text>0.13inch diam.
Clears 4-40 screw</text>
<text>Standard</text>
<text>Continuous Rotation</text>
<text>V11</text>
<text>Byron Jacquot</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
<package name="OSHW-LOGO-M">
</package>
<package name="SFE_LOGO_NAME_.2">
</package>
<package name="SFE_LOGO_FLAME_.2">
</package>
<package name="FIDUCIAL-1X2">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-2-NO_YES_SILK">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="PAD.03X.04">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-SMD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
<package name="1X02_NO_SILK">
</package>
<package name="1X03_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO14">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TRIMPOT_5MM">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="frame"/>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE" value="10K"/>
</element>
<element name="JP9" library="SparkFun-Connectors" package="2X3" value=""/>
<element name="U1" library="SparkFun-DigitalIC" package="SO14" value="ATTINY84">
<attribute name="PROD_ID" value="IC-11285"/>
</element>
<element name="R1" library="SparkFun-Electromechanical" package="TRIMPOT_5MM" value="10k">
<attribute name="PROD_ID" value="RES-11156"/>
</element>
<element name="R2" library="SparkFun-Electromechanical" package="TRIMPOT_5MM" value="10k">
<attribute name="PROD_ID" value="RES-11156"/>
</element>
<element name="R3" library="SparkFun-Electromechanical" package="TRIMPOT_5MM" value="10k">
<attribute name="PROD_ID" value="RES-11156"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="JP2" library="SparkFun-Connectors" package="1X03_NO_SILK" value="SERVO-OUT"/>
<element name="JP3" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="SFE_LOGO_NAME_.2" value="SFE_LOGO_NAME.2_INCH"/>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE" value="10K"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE" value="10K"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="N.O."/>
<element name="SJ2" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="N.O."/>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="RESONATOR-SMD" value="16MHZ">
<attribute name="PROD_ID" value="XTAL-08900"/>
</element>
<element name="STANDOFF1" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF4" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP4" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="LOGO3" library="SparkFun-Aesthetics" package="SFE_LOGO_FLAME_.2" value="SFE_LOGO_FLAME.2_INCH"/>
<element name="TP1" library="SparkFun-Passives" package="PAD.03X.04" value="TEST-POINT3X4"/>
<element name="TP2" library="SparkFun-Passives" package="PAD.03X.04" value="TEST-POINT3X4"/>
<element name="TP3" library="SparkFun-Passives" package="PAD.03X.04" value="TEST-POINT3X4"/>
<element name="FID1" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FID2" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP9" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C1" pad="A"/>
<contactref element="R1" pad="C"/>
<contactref element="R3" pad="C"/>
<contactref element="R2" pad="C"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="14"/>
<contactref element="JP9" pad="6"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="SJ1" pad="1"/>
<contactref element="SJ2" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="C"/>
<contactref element="Y1" pad="2"/>
<contactref element="R1" pad="A"/>
<contactref element="R3" pad="A"/>
<contactref element="R2" pad="A"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="MOSI/PWM">
<contactref element="U1" pad="7"/>
<contactref element="JP9" pad="4"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="8"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="9"/>
<contactref element="JP9" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="JP9" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="3"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="2"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="T">
<contactref element="R3" pad="B"/>
<contactref element="U1" pad="6"/>
<contactref element="TP3" pad="P$1"/>
</signal>
<signal name="B">
<contactref element="R2" pad="B"/>
<contactref element="U1" pad="10"/>
<contactref element="TP2" pad="P$1"/>
</signal>
<signal name="A">
<contactref element="R1" pad="B"/>
<contactref element="U1" pad="13"/>
<contactref element="TP1" pad="P$1"/>
</signal>
<signal name="BTN">
<contactref element="U1" pad="12"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="MODESEL">
<contactref element="U1" pad="5"/>
<contactref element="R5" pad="1"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="POLSEL">
<contactref element="U1" pad="11"/>
<contactref element="SJ2" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
